Appendix A

PLATFORM INFRASTRUCTURE

In this appendix the technical details of the many-screen platform infrastructure are outlined. The infrastructure offers client and server code that can be extended to implement the functionality required for a specific application. The modular code design and use of the model view controller pattern allow for this extensibility and easy code maintenance. The framework was utilised by the MarathOn Multiscreen Application.

# COMPONENTS

The platform consists of two main components the server and base code for application clients. Clients, which import the base code responsible for implementing the functionality listed below, can operate in one of two modes, either application or television. The mode is selected by the inclusion of a <DIV> element, in the applications main HTML file. The DIV element is given a class attribute of either ‘appWindow’ for applications, or ’tvWindow’ for television. Where an instance has been designated as television, the application launches a fullscreen video player view and playhead progress is propagated to all other connected clients and to the server to implement video feed resume functionality across the devices. In the current implementation of the platform, only a single client can be registered as a television. Clients running in application mode offer the remainder of functionality below, with code to implement the playback and scrubbing of video, channel and feed selection, television control, and display of interactive feeds. In addition, the underlying code structure allows for implementing clients to extend this functionality through the creation of new modules, implementing code specifically for that application’s requirements. Modules constructed for the MarathOn Multiscreen application, which implement a playlist across the connected devices, the runner interfaces and interact with the RunSpotRun dataset are described in the MarathOn Multiscreen Modules subsection below.

The server component is responsible for the connection and disconnection of clients, distributing a schema of channels to newly connected clients and logging user interaction across the devices. In addition the server maintains playheads for each video feed played on a client instance, which has been setup as a television. Therefore when new application clients are registered they can be informed of where the television feed has played to. This allows clients connecting after there has been some playback on the television, to accurately display statistical and information updates without revealing spoilers and correctly resuming playback.

# FUNCTIONALITY

The platform implemented the following functionality, which can be utilised in implementing applications.

***Core Functionality is Extendable****:* The platform implements core functionality common to both the Olympics and Marathon Application, as described by this list of requirements. However the platform is implemented using a modular design and the observer pattern (described in the Design Patterns subsection), so that additional functionality, specific to a particular application, is easily incorporated.

***Connection and Disconnection:***Application instances that implement the platform can connect and disconnect to the server at anytime during execution, therefore clients that connect after viewers have watched video on the television are able to resume playback of the feed at the correct playhead. In addition the server can support connection from any number of clients and can handle unexpected disconnection and reconnection because of crashes or accidental application closure by users.

***Download a schema of channels and feeds:*** Similarly to the Olympics Companion System, upon connection, the server provides a client with a schema of channels and feeds that are utilised by the application, the schema is encoded in JSON (JavaScript Object Notation). Logically content is divided into channels that contain feeds. Feeds can either be video or interactive content. Video feeds contain a URI to a video object, a name, description and thumbnail, and fields that dictate the times it is available to the user. Interactive feeds, referred to in the schema as TIC feeds, include the same fields as a video feed, with the exception of the video URI that is replaced by a list of URIs to web page content. Additionally interactive feeds can be paired with video feeds, allowing for synchronised playback with a video, facilitating stats and information functionality as seen in the Olympics Companion system. To complete the implementation of that functionality, the feed also contains a list view flag, when enabled users can switch between available pages and each page has an availability time associated with it. The schema used by MarathOn Multiscreen is described in the Application content section below and the utilised schemas for both studies are available in appendix B.

***Live Playhead:***Similar to the Olympics Companion System the code base implements a live playhead for each of the video feeds available in the channel schema. The live playhead mimics the notion of a broadcast by the playhead increasing as time passes, since the feed was made available to the user. Therefore if a user was to select a feed to playback live, 5 minutes after the feed was made available, the feed would start to playback 5 minutes into the video. The live playhead was not utilised by the MarathOn Multiscreen application, as the content used didn’t lend itself to being presented as a broadcast, the functionality was however implemented to achieve compatibility with the Olympics Companion System.

***Logging:*** All user interaction is logged to the server using a consistent protocol, (also utilised by the applications message bus and observer module). The application also builds on problems with logging in the Olympics application, caused by browser native HTML5 video controls, through implementation of custom video playback controls.

## Television Functionality

The following functionality is specific to application instances operating in the television mode:

***Play a video feed*:** Playback video feeds as initiated by user selection on application clients. Playback on the television application replicates the experience of watching broadcast television by displaying the video fullscreen and hiding all browser chrome from the user.

***On-Screen Notifications:***The television application displays simple on screen notifications to users, confirming feed changes, pausing, and fast forwarding and rewinding. This requirement is in response to the lack of television notifications that troubled users in the Olympics Application Study.

## Application Functionality

Finally, the following functionality is implemented by instances of the code base that operate in the application mode. It is expected that applications in this mode will be run on tablet devices.

***List channels and feeds:***Enumerate the channels and feeds that are described by the schema distributed by the server. Users can select feeds and channels from this list for playback on the tablet and television. A simplified version of this list functionality, along with the television controls described below, could be utilised in the development of a remote control application for functional equivalence with the Olympics Companion application.

***Instigate video playback:***Video feeds that are select by users from the feeds list can be played back on both the television and the tablet application. Subsequently, users have the option to select whether to begin this playback, from the beginning, from the live playhead or to resume previous progress from the television or the tablet. If both tablet and television have consumed part of the video, the higher playhead value will be selected to resume from. For example, if the television had played back a video feed from the start to 5 minutes and the tablet from the 5 minutes to 10 minutes, the tablets playhead would be selected to continue playback from 10 minutes.

***Playback video:*** Application instances can playback video in addition to television instances, enabling the parallel viewing user behaviour observed in the Olympics Companion user trial. The video player implementation in the Olympics Companion used the browser default controls, this generated issues with interaction logging, particularly when users scrub through the video, generating numerous seek interactions, which don’t accurately reflect a users intention. Therefore video player module implements custom video controls, which override the browser default controls.

***Interactive content:***Interactive feeds of content can be instigated and executed from within the clients identified as applications. In the Olympics Companion application and information feeds provided by the MarathOn Multiscreen application, these feeds consist of a series of a series of static HTML content. These pages can be enumerated in a user selectable list allowing users to select between available statistic updates. Functionality, such as the runner map and playlist in the MarathOn Multiscreen application, which offer more complex interactive experiences, are implemented by an interactive feed consisting of a single file of content. The file contains an HTML DIV element with a class or ID field that is recognised by a custom code module that implements the required functionality. This technique could enable the development of a range of unique applications, such as quiz shows and interactive narratives.

***Control the television*:** User control of the television is conducted through tablet applications. Using these controls viewers can pause and resume the video feed playing on the television, and fast-forward and rewind.

The following subsections describe how this functionality has been implemented in modules, using a message bus protocol and a series of design patterns. The Application Walkthrough section describes in detail the implementation of the platform for the marathOn Multiscreen system.

# DESIGN PATTERNS

To aid code reuse and organisation the following design patterns were utilised in the development of the multiscreen prototyping platform that the marathOn Multiscreen application is built upon:

***JavaScript revealing module pattern:***JavaScript doesn’t provide mechanisms for code separation or package syntax, the module pattern allows for code to organised into self-contained functional units that can be added, replaced or removed (Stefanov, 2010). A module is declared as an immediate function that returns an object this enables public and private scope, code declared in the return object has public scope and can be accessed by other modules. In the revealing version of the pattern all methods are declared in private scope but exposed in the return object (Stefanov, 2010). The division of code into modules supports easier code maintenance and application specific functionality without altering the core code base. The scoping provisions of the module pattern ensure that the core functionality of the platform is accessed safely by an implementing application. For a list of the platform’s core modules, and application specific models used in the MarathOn Multiscreen application see the Modules section below.

***Observer Pattern*:** The observer pattern (otherwise known as the publisher/subscriber module) defines a one-to-many dependency between modules. Such that when communication messages are received, a single update is made to the applications state and all other modules are notified of the change automatically (Gamma et al., 1995). For example the communication messages could derive from user interaction, receiving the channel schema, or playhead updates from other clients of the application. The pattern works by observers (in this instance the core and application specific modules) registering a callback function with the subject module. When an update is made to the applications data model the subject iterates through it’s list of observer callback functions and publishes a message informing the module of the model change. Therefore the subject is decoupled from the implementation and number of modules, it is up to the observing module to decide if the message is of use or if it should be discarded. The messages used in the platform to inform observer modules of changes to the model are the same The central application module exposes several functions to allow other modules to safely request update to the data model, which turn cause the subject module to iterate a message through to it’s subscribers. The following code snippet shows the implementation of a module and its observer callback function.

var demo = (function()

{

moduleName = “demoModule";

var observerCallback = function(message){

if(message == "ready")

{

privateFunction();

}

}

app.subscribe(moduleName, observerCallback);

var privateFunction = function(){

console.log(“this is the private function”);

}

var publicFunction = function(){

Console.log(“This is a public function”);

}

return{

publicFunction: publicFunction

}

}());

The demo module implements three functions the obseverCallback function is registered with the observer patterns subject using the call to app.subscribe(moduleName, observerCallback). When the observerCallback function receives a message from the subject it is compared with the message ‘ready’, if the condition is matched the privateFunction is called and displays a message to the browser console. The final function, publicFunction is made available to other modules in the application by including a reference to it in the return object.

***Model-View-Controller****:* The model-viewer-controller pattern (abbreviated to MVC) is implemented using the Observer pattern and ensures division between the underlying data model used by the application and it’s presentation to the user, using controller objects or modules as a go between (Gamma et al., 1995). Again the MVC pattern helps making code readable and extendable. The platform’s model has two parts an application model, which is received from the server at runtime, and the internal model, derived from the application model but is updated with playhead values and application specific functionality. The majority of modules are controllers communicating with the application and internal models using their observer callback functions, handling user interactions with the application or responding to playhead events. Application views are implemented using a templating language, in this case EJS (EJS - JavaScript Templates, 2014). JavaScript templating allows for executable code to be included in HTML markup, therefore the views are dynamically generated at runtime in easily maintainable code separate from the controller modules. The following diagram shows the relationship between model and controller modules, and templated views in the multiscreen platform.




Image A - 1 Multiscreen platform architecture overview

# PLATFORM MESSAGING PROTOCOL

Application instances and the server communicate using a message bus, this replaces the long polling techniques used by the Olympics application with a more robust and scalable method of communication. A proprietary message bus, Apache Apollo (Apollo, 2014), is used to broker transmission between components. Platform specific messages are wrapped in the Simple text orientated messaging protocol (abbreviated to STOMP) (STOMP, 2012) that defines client connection and disconnection (to the message bus not the applications server), and message routing. Apollo was chosen as it allows connection natively over web sockets to the web based clients of the application, however Apollo could be replaced with any future product, supporting web sockets and STOMP, and function identically. The following table outlines the message types used by the platform and how they enable the core functionality utilised by the MarathOn Multiscreen application. The communication messages are transmitted across the message bus, in the body section of the STOMP frame, they are encoded in JSON.

|  |  |  |
| --- | --- | --- |
| **Message Type** | **Description** | **Example** |
| newConnection | A request from the client to the server to connect. Upon a successful request the server responds with the data message. The connection request also includes the device type either app or television. | {"type":"connection", "connectionType": "newConnection”, “deviceType":"app"} |
| connectionAccept | Response to the server to a connection request, includes a unique identifier for the client and the channel schema for the application to use. Further communication from the client utilises the identifier, so the sever knows how to deal with communication from each client, for example if the client is registered as a television, it updates the servers internal model of television playheads. Additionally all messages include a timestamp, therefore logs have temporal information and nodes can interpret the order of messages correctly. | {“type”:”connectionAccept”, ”deviceId":1416494176508, "data":{"app":[{...}]}, "timestamp":1416493965553} |
| Disconnection | A request from the client to the server to disconnect. | {"type": "connection", "connectionType": "disconnect", "deviceID":1416494176184, "deviceType":"tv"} |
| Ready | A simple internal message not sent across the message bus informing observing modules that the application and internal models has been setup based on the data received from the server. | “ready" |
| StatusUpdate | User initiated changes to the applications state such as changing the channel or selecting a video feed. In the example opposite, the user has selected the professional video feed, which has the ID ‘raceOverviewVideo’ and the playback location is start. The progress field refers to any progress that the user has already made in the video stream, should the location be resume. In this case it is the first time the video has been played and the progress is set to 0. | {"statusUpdate":{"type":"feedSelect", "device":"app”, “ feedId":"raceOverviewVideo", "progress":0, "location":"start"},"timestamp":1416494240901,"deviceId":1416494176508} |
| PlayheadUpdate | Changes to the playhead state, such as fast forward, rewind and pause. Playhead time updates, raised by the HTML5 video time update method are generated approximately every 200ms, therefore to avoid unnecessary overhead are sent locally, to other observers but not sent across the message bus. This is indicated by the headOnly flag. Other application instances maintain their own playhead clock for the television, responsive to other playheadUpdates and occasional sync updates every 10 seconds. The state field indicates if the video player is paused or playing back and the seeker flag is set to true when the user has fast forwarded or rewound the video feed. | {"playheadUpdate":{"headOnly":false,"feedId":"raceOverviewVideo”, “progress":5.525578,"state":"paused”, “seeked":false,"eventsViewed":[]},"timestamp":1416494247194,"deviceId":1416494176508} |
| App | The app message type is left for application specific messages. For example, in the MarathOn Multiscreen, the first example opposite adds a new tag to the RunSpotRun dataset, including the tags location along the course (calculated from the latitude and longitude), the runners bib number, the time in the video and identifiers for the spectator and video. | Add new tag  {“app":{"type":"newTag”, “tag":{"distance":9412,"id":"1416494558647454”, “latitude":52.933254480440056,"longitude":-1.20449899647435,"raceNo":"1134”, “spectatorID":"dcb42e4e-7196-4d11-837a-9b8aac8a3e8c”, “time":1380445760.680195,"videoID":"896c3537-c43b-4ed2-a804-d2f1c58fbefc"}},"timestamp":1416494347362,"deviceId":1416494176508}  Add video to playlist:  {"app":{"type":"update”, “playlist":[{"feedId":"spectatorp9Video”, “startTime":1433,"endTime":1483,"playlistId":"14164946163710”, “thumbnail":"http://192.168.0.2/multiscreenWebappMarathon/imgs/thumbs/p9Video.png”, “feedName":"spectator 9 videos"}]},"timestamp":1416494405086,"deviceId":1416494176508} |

Table A - 1 Multiscreen platform message types

# MODULES

The following table outlines the modules implemented by the multiscreen platform and those implemented specifically for the MarathOn Multiscreen application.

|  |  |  |
| --- | --- | --- |
| Server Core Modules | | |
| Module Name | Module Description | |
| Connection | Handle incoming connections and disconnections from clients, including distributing the channel schema. | |
| Logging | Log user interactions from the message bus into a persistent file. | |
| main | Main module which kicks off the server and handles loading in of persistent channel schema defined by a command line argument. | |
| tvPlaybackState | Maintain the playback status of each channel for the television client. | |
| MarathOn Multiscreen Server Modules | | |
| playlistServer | Maintains the state of the playlist as an ordered array of videos. | |
| Core Modules | | |
| App | The application module stores the application and instance models. It is also responsible for providing other modules safe access to the models and implements the subject for the observer pattern.  In addition the app module is the entry point for the application and kick start connection to the message bus. | |
| Availability | The availability module determines which channels and feeds are available to users at any given time during the clients execution. Therefore feeds which have a start time and end time set are only available to users at the appropriate time. | |
| ChannelList | Controller module that handles display and interaction with the channel list and feed selection. | |
| MessageBus | Interface between the Message bus, the client and server. This module handles connection and disconnection to the message bus and server, and passes incoming messages to the application module and outgoing messages to the bus. | |
| Observer | Handles subscription and unsubscription of modules to the subject (application module), publishes messages to subscribing modules. | |
| SyncTime | The SyncTime module provides a synced time with the server, so playhead calculations of other clients are accurate. The syncTime is calculated by requesting a time from the server at the start of the clients execution and adjusting for network latency. All subsequent requests for a time value are calculated as a delta from the requested server time. | |
| TICPageList | Enumerate the HTML pages available in an interactive feed and handle user interaction by issuing a playheadUpdate message to the observer subject to be handled by the TICPlayback module. | |
| TICPlayback | Controller module that displays the selected interactive feed page. | |
| TVControls | Controller module that displays the TV controls on an application client and handles user interaction with them, issuing playhead update messages to be sent across the bus. | |
| TVOverlay | Module to handle the display of information overlays on the television client, such as pause notifications and channel changes. | |
| TVPlayback | Responds to user interactions on application clients to playback and control the playback of video feeds on the television. | |
| TVStatus | The TVstatus module is used by clients operating in application mode. The module maintains the playhead status of a TV client. | |
| VideoPlayback | Controller module which handles playback and user interaction of video feeds on application clients. | |
| MarathOn Multiscreen Modules | | |
| eventPlaybackButton | | Handler for buttons that allow for the playback of a single event, such as a runner appearing in a video, the video ID, and the playhead locations for the start and end of playback are encoded in the buttons ID. This module extracts the values from the ID and tells the message bus to playback video from start to end playheads |
| RunnerMap | | Controller module which displays and handles interaction with the runner map view. |
| marathonHelpers | | A series of helper functions specific to functionality implemented by the marathOn Multiscreen application. Including  Get videos that a particular runner is either in or is possibly in. This is calculated by a runners speed between two known points, either the start or end of the race, or other video tags, and cross referencing with the time each video was taken.  Get and set methods for the RunSpotRun data file.  A playback dialog, allowing users to select whether to watch a short clip of the runner on either the television or the tablet, or to add it to the playlist. |
| taggingInterface | | Controller module for a interactive feed page from which users can tag runners on the television. |
| PlaylistAddButton | | Controller module, which handles user interaction with a button which adds videos to the playlist. playlist buttons are implemented by assigning a button or div control the class name ‘addToPlyalistButton’ |
| Playlist | | Controller module to handle display and user interactions with the playlist interactive feed page. |
| RunnerList | | Controller module which displays and handles interaction with the runner list view. |
| TabletTagOverlay | | An overlay applied to applications clients video playback display that implements a runner tag button. |

Table A - 2 Multiscreen platform messages